WARNING: REI recommends using fully charged batteries during the ANDRE firmware update process. Without sufficient power there is a risk of the ANDRE losing power during the update and rendering the unit inoperable.

Updating the firmware on your ANDRE unit:
1.  Connect the ANDRE to a PC using the included USB A to USB Micro B cable.
2.  The computer should recognize the ANDRE and represent it as a drive similar to how a USB thumb drive would be represented.
3.  Transfer the .bin firmware update file to the root directory on the ANDRE.
4.  Once the file has successfully transferred to the ANDRE, disconnect the ANDRE from the computer.
5.  The ANDRE will recognize there is a new update file and prompt the user to install.
6.  During the update process, the ANDRE will perform a soft reset.
7.  Once the update is complete, perform a full shutdown and reboot using the power button.
8.  ANDRE is ready to use.

*Note: The ANDRE will delete the update .bin file from its storage once the update has been performed.

